**Guidelines for restoring BBNL OFC having more than 500 metre cuts.**

**Mandatory Points**

* Reimbursement towards the material of PLB duct and OFC should be limited to current/latest tendered discovered costs of these by BSNL/PGCIL/Railtel
* PLB duct and OFC must be used of same specification
* Markers must be installed at the time of restoration
* Trenching, laying, and jointing work of PLB/OFC must be administered by applicable Engineering Instructions

**Note: Please submit the details as per below given format:**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **District** | **Block** | **Name of affected GPs** | **Proposed OFC length of replacement** | **Lat-Long of Both end** | **OTDR reading from Both end** | **Effort taken to ascertain damaged length** | **Reason of damage** |
|  |  |  |  |  |  |  |  |

* **OTDR Traces**
* **Lat-Long of Route**